{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet2"],"not_rendered":{"images":8,"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"Sheet2","index":0,"n_rows":35,"n_cols":11,"rows_kept":35,"merged":[[0,0,0,10],[1,0,3,0],[1,1,3,1],[1,2,3,2],[1,3,3,3],[1,4,3,4],[1,5,3,5],[1,6,1,8],[1,9,3,9],[1,10,3,10],[2,6,3,6],[2,7,3,7],[2,8,3,8],[7,5,8,5],[7,10,8,10],[29,0,29,6],[29,7,29,8],[30,0,30,10],[31,0,31,5]]}
["2023年“H”项目灯具采购报价表"]
["序号","项目名称","项目特征描述","数量","计量\r\n单位","选型照片","金额（元）",null,null,"报价品牌","质量要求"]
[{"$nulls":6},"全费用单价限价","供应商所报单价","合价"]
[]
[1,"45W/LED 庭院灯","尺寸：400*400*4000mm  内置LED光源                \n材料：铝合金型材 壁厚2.5mm                                光源：LED45W  \n电压：AC220V，色温：3000K\n防护等级：IP65",150,"套",{"$f":"_xlfn.DISPIMG(\"ID_C52E72E7742D473EA82CAFA294AFFD74\",1)","v":"=DISPIMG(\"ID_C52E72E7742D473EA82CAFA294AFFD74\",1)"},2000,{"$nulls":3},"LED光源和灯具均不低于雷士、飞利浦、欧普的品牌品质要求，含预埋件"]
[2,"18W/LED 草坪灯","尺寸：150*150*800mm 内置LED光源                     材料：铝合金型材 壁厚1.5mm                           光源：LED10W \n电压：AC220V，色温：3000K\n防护等级：IP65       ",73,"套",{"$f":"_xlfn.DISPIMG(\"ID_55737057EDF24F28B04E005E4D3B5F28\",1)","v":"=DISPIMG(\"ID_55737057EDF24F28B04E005E4D3B5F28\",1)"},450,{"$nulls":3},"LED光源和灯具均不低于雷士、飞利浦、欧普的品牌品质要求，含预埋件"]
[3,"36W/LED 投光灯","材质：压铸铝灯体 功率：36W \n电压：AC220V 光通量：3500lm，色温：3000K\n防护等级：IP65",66,"套",{"$f":"_xlfn.DISPIMG(\"ID_706ABC6B5310406789E8859C8EC88FBA\",1)","v":"=DISPIMG(\"ID_706ABC6B5310406789E8859C8EC88FBA\",1)"},330,{"$nulls":3},"LED光源和灯具均不低于雷士、飞利浦、欧普的品牌品质要求，含3mm厚30*30角钢安装基础"]
[4,"5W/M/LED 柔性灯带","外皮材质：透明硅胶     \n尺寸：12*5mm 功率：5W/米 120珠，搭配20*15铝合金铝材 \n电压：DC24V，色温：3000K\n防护等级：IP68",2795,"米",{"$f":"_xlfn.DISPIMG(\"ID_583D7AD0B09C49FE8FD1CA488BF36DB4\",1)","v":"=DISPIMG(\"ID_583D7AD0B09C49FE8FD1CA488BF36DB4\",1)"},22,{"$nulls":3},"LED光源和灯具均不低于雷士、飞利浦、欧普的品牌品质要求，含不锈钢卡口、灯槽等安装辅件"]
[5,"10W/M/LED 柔性灯带","外皮材质：透明硅胶     \n尺寸：12*5mm 功率：10W/米 120珠，搭配20*15铝合金铝材 \n电压：DC24V，色温：4000K\n防护等级：IP68",840,"米",null,24]
[6,"48W/1M/LED 洗墙灯","规格：1000mm      功率：48W\n产品材质：定制压铸铝外壳+钢化玻璃+双层密封\n电压：DC24V，色温：RGB+W\n防护等级：IP68",380,"套",{"$f":"_xlfn.DISPIMG(\"ID_144FCA8D97134FB19C00D823277749C3\",1)","v":"=DISPIMG(\"ID_144FCA8D97134FB19C00D823277749C3\",1)"},480,{"$nulls":3},"LED光源和灯具均不低于雷士、飞利浦、欧普的品牌品质要求，水池四周"]
[7,"24W/0.5M/LED 洗墙灯","规格：500mm      功率：24W\n产品材质：定制压铸铝外壳+钢化玻璃+双层密封\n电压：DC24V，色温：RGB+W\n防护等级：IP68",2,"套","=DISPIMG(\"ID_144FCA8D97134FB19C00D823277749C3\",1)",420,{"$nulls":3},"LED光源和灯具均不低于雷士、飞利浦、欧普的品牌品质要求，水池四周"]
[8,"15W/0.3M/LED 洗墙灯","规格：300mm      功率：15W\n产品材质：定制压铸铝外壳+钢化玻璃+双层密封\n电压：DC24V，色温：RGB+W\n防护等级：IP68",2,"套","=DISPIMG(\"ID_144FCA8D97134FB19C00D823277749C3\",1)",360,{"$nulls":3},"LED光源和灯具均不低于雷士、飞利浦、欧普的品牌品质要求，水池四周"]
[9,"24W/1M/LED 洗墙灯","规格：1000mm        功率：24W\n产品材质：定制压铸铝外壳+钢化玻璃+双层密封\n电压：DC24V，色温：3000K\n防护等级：IP65",686,"套",{"$f":"_xlfn.DISPIMG(\"ID_4A1F2D19CA0443B49CBFBD71AF5A90F9\",1)","v":"=DISPIMG(\"ID_4A1F2D19CA0443B49CBFBD71AF5A90F9\",1)"},130,{"$nulls":3},"LED光源和灯具均不低于雷士、飞利浦、欧普的品牌品质要求，景墙,含3mm厚30*30角钢安装基础"]
[10,"12W/0.5M/LED 洗墙灯","规格：500mm        功率：12W\n产品材质：定制压铸铝外壳+钢化玻璃+双层密封\n电压：DC24V，色温：3000K\n防护等级：IP65",5,"套",{"$f":"_xlfn.DISPIMG(\"ID_4A1F2D19CA0443B49CBFBD71AF5A90F9\",1)","v":"=DISPIMG(\"ID_4A1F2D19CA0443B49CBFBD71AF5A90F9\",1)"},110,{"$nulls":3},"LED光源和灯具均不低于雷士、飞利浦、欧普的品牌品质要求，景墙,含3mm厚30*30角钢安装基础"]
[11,"8W/0.3M/LED 洗墙灯","规格：300mm           功率：8W\n产品材质：定制压铸铝外壳+钢化玻璃+双层密封\n电压：DC24V，色温：3000K\n防护等级：IP67",8,"套",{"$f":"_xlfn.DISPIMG(\"ID_9357E93705B04005941960C4A45C0FF2\",1)","v":"=DISPIMG(\"ID_9357E93705B04005941960C4A45C0FF2\",1)"},95,{"$nulls":3},"LED光源和灯具均不低于雷士、飞利浦、欧普的品牌品质要求，1-4#洗墙灯"]
[12,"350W//LED 激光灯","输入电压：AC90-240V 50-60Hz\n整机功率:350W\n光源理论寿命 1500小时以上\n灯泡色温: 7800K\n调    焦 :线性电动调焦\n调    光 :调光平滑无闪烁\n镇 流 器 :优灯\n频    闪 :独立频闪、0.5-20次/秒可调\n电压：AC220V\n防护等级：IP65",6,"套",{"$f":"_xlfn.DISPIMG(\"ID_043863A767EC40E3A265D2198F35B783\",1)","v":"=DISPIMG(\"ID_043863A767EC40E3A265D2198F35B783\",1)"},7500,{"$nulls":3},"LED光源和灯具均不低于雷士、飞利浦、欧普的品牌品质要求，含安装基础,2米高,3mm厚50*50角钢安装支架 "]
[13,"配电箱L1","室外落地式配电箱 / 不锈钢 304 材质 / 防护等级 IP54，具体详见图纸",1,"台",null,17000,{"$nulls":3},"元器件不低于西门子、ABB、施耐德的品牌品质要求"]
[14,"配电箱L2","室外落地式配电箱 / 不锈钢 304 材质 / 防护等级 IP54，具体详见图纸",1,"台",null,17000,{"$nulls":3},"元器件不低于西门子、ABB、施耐德的品牌品质要求"]
[15,"配电箱L3","室外落地式配电箱 / 不锈钢 304 材质 / 防护等级 IP54，具体详见图纸",1,"台",null,11000,{"$nulls":3},"元器件不低于西门子、ABB、施耐德的品牌品质要求"]
[16,"配电箱L4","室外落地式配电箱 / 不锈钢 304 材质 / 防护等级 IP54，具体详见图纸",1,"台",null,12000,{"$nulls":3},"元器件不低于西门子、ABB、施耐德的品牌品质要求"]
[17,"配电箱L5","室外落地式配电箱 / 不锈钢 304 材质 / 防护等级 IP54，具体详见图纸",1,"台",null,8000,{"$nulls":3},"元器件不低于西门子、ABB、施耐德的品牌品质要求"]
[18,"配电箱L6","室外落地式配电箱 / 不锈钢 304 材质 / 防护等级 IP54，具体详见图纸",1,"台",null,8000,{"$nulls":3},"元器件不低于西门子、ABB、施耐德的品牌品质要求"]
[19,"配电箱L7","室外落地式配电箱 / 不锈钢 304 材质 / 防护等级 IP54，具体详见图纸",1,"台",null,8000,{"$nulls":3},"元器件不低于西门子、ABB、施耐德的品牌品质要求"]
[20,"防水开关电源","320W/AC220V/DC24V 功率因数不小于 0.9 ,IP68，保护功能:短路、过载、过压、过温",480,"套",null,180]
[21,"主控器","DMX512 系统、脱机主控、千兆网口 *2 、 TCP/IP 协议",1,"套",null,5000]
[22,"分控器","DMX512 系统、 8 个 LED 带载输出端口、千兆网口 *2 、 TCP/IP 协议",7,"套",null,2000]
[23,"交换机","16口网络交换机",1,"套",null,750]
[24,"激光灯控台","DMX512,舞台灯光控台",1,"套",null,5000]
[25,"防水网线","FS-CAT6E",5685,"米",null,3]
["合计（大写：                                            ），能开具税率：            ",{"$nulls":6},{"$f":"SUM(I5:I29)","v":0}]
["注：1.要求报价为含税到场价，开具的发票为1%税率或3%税率或13%税率的增值税专用发票。"]
["    2.所有灯具须符合相关行业质量标准，以实际供应数量按实结算。"]
[null,"                                       ",{"$nulls":4},"报价单位（公章）："]
[{"$nulls":6},"委托代理人及电话："]
[{"$nulls":6},"时间：      年    月    日"]